3200 Series (Z-Wave™ Door) User’s Command Manuals
                        Date:2022/02/17
一.Reverting to Factory Setting
The lock memory can be cleared and made to revert to the factory Master Code as follows:

1. Remove one battery.

2. Press and hold the ‘0’ button, replace the battery, the Blue LED will flash twice, beep will sound twice at the same time, then release the ‘0’ button.

3. Within 3 seconds press the ‘*’ button 3 times. The Blue LED will light continuously for 7 seconds and 2 beeps will sound. The lock will have reverted to the factory, and all other settings will be erased.


※ Important: If you do not see Blue LED light continuously for 7 seconds and hear 2 beeps, you must start over at step 1.
二. Command Table:

	Function No.
	Function
	Program

	00
	Z-Wave™ Pairing and Z-Wave™ Reset

	Z-Wave™ Pairing ：# [Master Code or Sub-Master Code] ●0 0● 00 ●●(If it is loading default settings, it must change the Master Code before using other functions.)
Z-Wave™ Reset ：# [Master Code or Sub-Master Code] ●0 0● 99 ●●(If it is loading default settings, it must change the Master Code before using other functions.)

	01
	Change Master Code
	# [Master Code]●0 1●[1-digit Code length]●[New Master Code]● [New Master Code] ●●(If it is loading factory default settings, it must change the Master Code before using other functions.)

	02
	Add or Change User Codes
	# [Master Code or Manager Code or Sub-Master Code] ●0 2 ● [2-digit Location] ● [New User/Office/Emergency Code] ●●

	03
	Deleting User Codes
	# [Master Code or Manager Code or Sub-Master Code] ● 03 ● [2-digit Location] ●●

	04
	Disable User Codes
	# [Master Code or Manager Code or Sub-Master Code] ● 04 ● [2-digit Location] ●●

	05
	Enable User Codes
	# [Master Code or Manager Code or Sub-Master Code] ● 05 ● [2-digit Location] ●●

	06
	Disable All User Codes
	# [Master Code or Sub-Master Code] ● 06 ●●

	08
	Enable All User Codes
	# [Master Code or Sub-Master Code] ● 08 ●●


Result: Re-enables all 100 User & 5 Manager Codes (Service Codes must be re-programmed).

# [Manager Code]● 08 ●●
Result: Re-enables all Users under that Manager.

	09
	Code Location Function
	# [Master Code or Manager Code or Sub-Master Code] ● 09 ●[Enter User Code to be located the digit location]●●
Result: 
1. At the start of the Next Free Code Location function, the lock will flash both the Blue and RED LEDs and will emit 2 beeps.

2. Display 2-digit numbers in order according to location.
3. To signify the end of the Code Location function, the lock will flash both the Blue and RED LEDs and will emit 2 beeps. If no free address is found, then the lock will emit one long beep (0.5 sec) with a Red LED.

	10
	Next Free Code Address Locator
	# [Master Code or Manager Code or Sub-Master Code] ● 10 ●●
Report Sequence:
1. At the start of the Next Free Code Location function, the lock will flash both the Blue and RED LEDs and will emit 2 beeps.

2. Display 2-digit numbers in order according to location. It only searches range from 00 to 99.
3. To signify the end of the Code Location function, the lock will flash both the Blue and RED LEDs and will emit 2 beeps. If no free address is found, then the lock will emit one long beep (0.5 sec) with a Red LED. 

	11
	Add/ Edit Sub-Master Code 
	# [Master Code] ● 11 ●[New Sub-Master Code]● [New Sub-Master Code] ●●

	12
	Delete Sub-Master Code
	# [Master Code] ● 12 ● 12 ●●

	21
	Add a single Service Codes 1
	# [Master Code or Manager Code or Sub-Master Code] ● 21 ● [Enter new Service Code] ●●
A single Service Code only can use once.

	22
	Add a single Service Codes 2
	# [Master Code or Manager Code or Sub-Master Code] ● 22 ● [Enter new Service Code] ●●
A single Service Code only can use once.

	23
	Add a single Service Codes 3
	# [Master Code or Manager Code or Sub-Master Code] ● 23 ● [Enter new Service Code] ●●
A single Service Code only can use once.

	24
	Add a single Service Codes 4
	# [Master Code or Manager Code or Sub-Master Code] ● 24 ● [Enter new Service Code] ●●
A single Service Code only can use once.

	25
	Add a single Service Codes 5
	# [Master Code or Manager Code or Sub-Master Code] ● 25 ● [Enter new Service Code] ●●
A single Service Code only can use once.

	30
	Delete All Service Codes
	# [Master Code or Manager Code or Sub-Master Code] ● 30 ● 30 ●●

	31
	Delete a single Service Code 1
	# [Master Code or Manager Code or Sub-Master Code] ● 31 ●●

	32
	Delete a single Service Code 2
	# [Master Code or Manager Code or Sub-Master Code] ● 32 ●●

	33
	Delete a single Service Code 3
	# [Master Code or Manager Code or Sub-Master Code] ● 33 ●●

	34
	Delete a single Service Code 4
	# [Master Code or Manager Code or Sub-Master Code] ● 34 ●●

	35
	Delete a single Service Code 5
	# [Master Code or Manager Code or Sub-Master Code] ● 35 ●●

	40
	Enable Passage Mode
	# [Master Code or Manager Code or Sub-Master Code] ● 40 ●●

	41
	Disable Passage Mode
	# [Master Code or Manager Code or Sub-Master Code] ● 41 ●●

	42
	Pass Time (Door Unlock)
	# [Master Code or Sub-Master Code] ● 42 ● [2-digit 02-20 seconds] ●●
Z-Wave™ Door：05-20 seconds（default is 05 seconds）

	43
	Enable Groups (Factory default)
	# [Master Code or Sub-Master Code] ● 43 ●●
Result: Managers restricted to controlling only those User Access Codes

	44
	Disable Groups
	# [Master Code or Sub-Master Code] ● 44 ●●
Result: All Managers can program all User Access Codes.

	51
	Add Manager Codes 1
	# [Master Code or Sub-Master Code] ● 51 ● [Enter new Manager Code] 

●[2-digit First location] ●[2-digit Last location] ●●

	52
	Add Manager Codes 2
	# [Master Code or Sub-Master Code] ● 52 ● [Enter new Manager Code] 
●[2-digit First location] ●[2-digit Last location] ●●

	53
	Add Manager Codes 3
	# [Master Code or Sub-Master Code] ● 53 ● [Enter new Manager Code] 

●[2-digit First location] ●[2-digit Last location] ●●

	54
	Add Manager Codes 4
	# [Master Code or Sub-Master Code] ● 54 ● [Enter new Manager Code] 

●[2-digit First location] ●[2-digit Last location] ●●

	55
	Add Manager Codes 5
	# [Master Code or Sub-Master Code] ● 55 ● [Enter new Manager Code] 

●[2-digit First location] ●[2-digit Last location] ●●

	60
	Delete All Manager Codes
	# [Master Code or Sub-Master Code] ● 60 ● 60 ●●

	61
	Delete a single Manager Code 1
	# [Master Code or Sub-Master Code] ● 61 ●●

	62
	Delete a single Manager Code 2
	# [Master Code or Sub-Master Code] ● 62 ●●

	63
	Delete a single Manager Code 3
	# [Master Code or Sub-Master Code] ● 63 ●●

	64
	Delete a single Manager Code 4
	# [Master Code or Sub-Master Code] ● 64 ●●

	65
	Delete a single Manager Code 5
	# [Master Code or Sub-Master Code] ● 65 ●●

	71
	Keystroke Sound Level: On
	# [Master Code or Sub-Master Code] ● 71 ● 1●● low
# [Master Code or Sub-Master Code] ● 71 ● 2●● middle
# [Master Code or Sub-Master Code] ● 71 ● 3●● high（default）

	73
	Keystroke Sound Level: Off
	# [Master Code or Sub-Master Code] ● 73 ●●

	77
	Set Z-Wave™ ID code for Random Service Function
	# [Master Code or Sub-Master Code] ● 77●[New ID code]● [New ID code] ●●
[The digit Code length is 12]

	91
	Lock / Unlocked Status Indicator

	# [Master Code or Sub-Master Code] ● 91 ● 1 ●● Result = No LED’s (default status)
# [Master Code or Sub-Master Code] ● 91 ● 2 ●● Result = Locked (Red LED flashing)
# [Master Code or Sub-Master Code] ● 91 ● 3 ●● Result = Unlocked (Green LED flashing)

	92
	Keypad Anti-Tamper Lockout
	# [Master Code or Sub-Master Code] ● 92 ● [1-digit invalid codes entry] ● [1-digit X0 seconds] ●●

	98
	Check Lock FW version
	# [Master Code or Sub-Master Code] ● 98●●
[The digit length of FW version is 3]

	99
	Reverting to Factory Setting
	# [Master Code] ●99 ● 99 ●● (7 seconds)
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