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The smart deadbolt lock by TLJ is wireless battery powered digital keypad. The smart deadbolt lock is based upon Z-WaveTM Slave Library V7.16.3 supporting numeric PIN codes and remote lock/unlock when connected to a Z-Wave gateway. It can be included and operated in any Z-Wave network alongside other Z-Wave certified devices from other manufacturers and/or applications. All non-battery operated nodes within the network will act as repeaters regardless of vendor to increase reliability of the network.
The smart deadbolt lock is a secure Z-Wave device (s0 & s2) so a security enabled controller is needed for take full advantage of all functionally for the Door Lock. It also supports over the air (OTA) firmware upgrades. In addition SmartStart and low battery alerts are also supported.
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Technical Specifications

	Communication Protocol
	Z-Wave (700Series)
	BLE (5.1)

	Radio Frequency
	908.42MHz  (US)
868.42MHz  (EU)
	2.4Ghz

	Wireless Range
	To Gateway:
More than 100m outdoors
Approx. 30m indoors (depending
on building materials)
	To Door Lock:
Max. 4m outdoors
Max 6m indoors

	Power Source
	Battery (6Volt 4 x LR6)

	Working current
	15mA

	Standby current
	30uA

	Battery Life
	~12 Months

	Operating Temperature
	32-104° F (0-40° C)

	Operating Humidity 
	8% to 85% non-condensing

	Certifications
	Z-Wave

	Dimensions (mm)
	Front: 132mm*98mm*57mm ;  Back: 100mm*68mm*41mm





Z-WaveTM Specifications

	SDK Version
	7.16.03

	SDK Library
	libZWaveSlave

	Explorer Frame Support
	Yes

	Routing
	Yes

	SmartStart
	Yes

	Device Type
	Lock

	Basic Device Class
	BASIC_TYPE_ROUTING_SLAVE

	Generic Device Class
	GENERIC_TYPE_ENTRY_CONTROL (0x40)

	Specific Device Class
	SPECIFIC_TYPE_DOOR_LOCK (0x01)

	Role Type
	Listening Sleeping Slave (LSS)
















Familiarize yourself with Door Lock
[image: 662 图片已改]

The smart deadbolt lock is a security enabled Z-Wave PlusTM product that is able to use encrypted Z-Wave Plus messages to communicate to other security enabled Z-Wave Plus products. When a node includes into a S0, S2 Z-Wave network, the node supports S0, S2Access and so do the supported CCs

Supported Security Levels
· SECURITY_KEY_S2_ACCESS_BIT
· SECURITY_KEY_S0_BIT

Commands List
	Command Classes
	Version
	Required Security Class

	COMMAND_CLASS_ZWAVEPLUS_INFO_V2
	2
	None

	COMMAND_CLASS_TRANSPORT_SERVICE_V2
	2
	None

	COMMAND_CLASS_SECURITY_V1
	1
	None

	COMMAND_CLASS_SECURITY_2_V1
	1
	None

	COMMAND_CLASS_SUPERVISION_V1
	1
	None

	COMMAND_CLASS_TIME_V2
	2
	None

	COMMAND_CLASS_NOTIFICATION_V8
	8
	S0 or S2 Access

	COMMAND_CLASS_DOOR_LOCK_V4
	4
	S0 or S2 Access

	COMMAND_CLASS_USER_CODE_V1
	1
	S0 or S2 Access

	COMMAND_CLASS_BATTERY_V1
	1
	S0 or S2 Access

	COMMAND_CLASS_CONFIGURATION_V4
	4
	S0 or S2 Access

	COMMAND_CLASS_ASSOCIATION_V2
	2
	S0 or S2 Access

	COMMAND_CLASS_ASSOCIATION_GRP_INFO_V1
	3
	S0 or S2 Access

	COMMAND_CLASS_VERSION_V3
	3
	S0 or S2 Access

	COMMAND_CLASS_MANUFACTURER_SPECIFIC_V2
	2
	S0 or S2 Access

	COMMAND_CLASS_DEVICE_RESET_LOCALLY_V1
	1
	S0 or S2 Access

	COMMAND_CLASS_POWERLEVEL_V1
	1
	S0 or S2 Access

	COMMAND_CLASS_FIRMWARE_UPDATE_MD_V5
	5
	S0 or S2 Access

	COMMAND_CLASS_MULTI_CHANNEL_ASSOCIATION_V3
	3
	S0 or S2 Access

	COMMAND_CLASS_INDICATOR_V3
	3
	S0 or S2 Access

	COMMAND_CLASS_TIME_PARAMETERS
	1
	S0 or S2 Access

	COMMAND_CLASS_BASIC
	2
	S0 or S2 Access

	COMMAND_CLASS_DOOR_LOCK_LOGGING
	1
	S0 or S2 Access

	COMMAND_CLASS_SCHEDULE_V1
	1
	S0 or S2 Access

	COMMAND_CLASS_SCHEDULE_ENTRY_LOCK
	3
	S0 or S2 Access



[bookmark: _Toc487807720][bookmark: _Toc484417913]All functions of each trigger



SmartStart Inclusion
SmartStart enabled products can be added into a Z-Wave network by scanning the Z-Wave QR Code present on the product with a controller providing SmartStart inclusion. No further action is required and the SmartStart product will be added automatically within 10 minutes of being switched on in the network vicinity.
Add the smart deadbolt lock into the Z-Wave network via SmartStart (SmartStart Inclusion):
a. Add smart deadbolt lock DSK into the primary controller SmartStart Provisioning List (DSK is printed on the back side of the smart deadbolt lock).
b. Please refer the user manual to trigger the smart deadbolt lock to enter learn mode for SmartStart inclusion.
c. The smart deadbolt lock will send “Z-Wave protocol Command Class” frame  to start SmartStart Inclusion.

Operating mode via Z-Wave™
All functions of each trigger



Onboard Menu
[image: 662 onboard menu]
Initially power on for the first time, touch the keypad,it will display “M”(number 1 3 4 5 6 7 9 light up) then “+”(number 2 4 5 6 7 8 light up). Input the first PIN code as master PIN (4 - 8 digit), then tap button “√”. The previous input PIN code will display on the keypad again as confirmation, then tap button “√” to confirm the master PIN code.  

Touch the screen and input two random code.  Hold the button “√” for 3 seconds,it will display “M”(number 1 3 4 5 6 7 9 light up). Later all keys are light up then input the master PIN. Later “number 1 2 9 0” will light up, tap “2” to enter into Z-Wave gateway paring mode. 

Ensure to enter the gateway into inclusion/exclusion mode at the same time. The Smart deadbolt lock will timeout after 60 seconds of inactivity. When inclusion or exclusion is finished The Smart deadbolt lock will sound audible beeps and returns to the main menu. 




Factory Reset
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Factory Reset :  Hold the Reset button(internal button) for 20seconds until the panel display number “1”and“2”, then release the button, then press “✔" button on front screen (the keypad LED will flash).
Reset all configurations to default status
Delete access for all users and user types
Delete the current Master PIN
Delete the current operating mode
Delete the directional handling
Gateway pairing deleted
Please use this procedure only when the network primary controller is missing or otherwise inoperable. 


  Z-Wave Plus Report Command Class



Manufacturer ID: TLJ smart deadbolt lock 0x0449 
Product ID: 0x0002 
Product Type ID: 0x00 04
Node Type: 0x00 (NODE_TYPE_ZWAVEPLUS_NODE)
Installer Icon Type: 0x0300 (ICON_TYPE_GENERIC_DOOR_LOCK_KEYPAD)
User Icon Type: 0x0300 (ICON_TYPE_GENERIC_DOOR_LOCK_KEYPAD)

  Supported Command Classes



Basic Command Class
[bookmark: _Hlk108009050]Basic Set (Value) maps Door Lock Operation Set (Door Lock Mode).
Basic get (Value) maps Door Lock Operation Get.
Basic Report (Current Value = 0x00) maps Door Lock Operation Report (Door Lock Mode = 0x00).
Basic Report (Current Value = 0xFF) maps Door Lock Operation Report (Door Lock Mode > 0x00).
  Association Command Class




	Grouping Identifier
	Max Nodes
	Send Commands

	Group 1(Lifeline Group)
	0x05
	1. NOTIFICATION_REPORT
The smart deadbolt lock will send NOTIFICATION_REPORT when access control or power management notification type triggered.
2. BATTERY_REPORT
The smart deadbolt lock will send BATTERY_REPORT when be unlocd.
3. DEVICE_RESET_LOCALLY_NOTIFICATION
Press and hold Reset Button more than 30s and when the button is released. The smart deadbolt lock will reset itself to factory default by sending a “Device Reset Locally Notification” to gateway.
4. USER_CODE_REPORT
The smart deadbolt lock will send USER_CODE_REPORT when user code changed.
5. DOOR_LOCK_OPERATION_REPORT_V4
The smart deadbolt lock will send DOOR_LOCK_OPERATION_REPORT when manual door lock operationed.
6. DOOR_LOCK_CONFIGURATION_REPORT
The smart deadbolt lock will send DOOR_LOCK_CONFIGURATION_REPORT when Door Lock configuration has changed.
7. INDICATOR_REPORT



  Notification Commands



	Notification Type
	Notification Event

	ACCESS_CONTROL (0x06)
	MANUAL_LOCK_OPERATION(0x01)
RF_LOCK_OPERATION(0x03)
RF_UNLOCK_OPERATION(0x04)
KEYPAD_LOCK_OPERATION(0x05)
KEYPAD_UNLOCK_OPERATION(0x06)
AUTO_LOCK_LOCKED_OPERATION(0x09)
ALL_USER_CODES_DELETED(0x0C)
SINGLE_USER_CODE_DELETED(0x0D)
NEW_USER_CODE_ADDED(0x0E)
NEW_USER_CODE_NOT_ADDED_DUE_TO_DUPLICATE_CODE(0x0F)
KEYPAD_TEMPORARY_DISABLED(0x10)

	POWER_MANAGEMENT (0x08)
	REPLACE_BATTERY_SOON(0x0A)
REPLACE_BATTERY_NOW(0x0B)
Previous Events cleared (0x00)



Access Control
MANUAL_LOCK_OPERATION(0x01):  when manual lock.
MANUAL_UNLOCK_OPERATION(0x02) :  when manual unlock.
RF_LOCK_OPERATION(0x03) : when used RF lock.
RF_UNLOCK_OPERATION(0x04) : when used RF unlock.
[bookmark: OLE_LINK4]KEYPAD_LOCK_OPERATION(0x05) : when used IC card lock.
KEYPAD_UNLOCK_OPERATION(0x06) : when used IC card unlock.
AUTO_LOCK_LOCKED_OPERATION(0x09) when auto lock
ALL_USER_CODES_DELETED(0x0C) when delete all user
SINGLE_USER_CODE_DELETED(0x0D) when delete single user
NEW_USER_CODE_ADDED(0x0E) : when New user code added.
NEW_USER_CODE_NOT_ADDED_DUE_TO_DUPLICATE_CODE(0x0F) : when New user code not added due to duplicate code.
KEYPAD_TEMPORARY_DISABLED(0x10) when keypad temporary disabled
Power Management:
REPLACE_BATTERY_SOON (0x0A): When the battery level is LOW.
REPLACE_BATTERY_NOW (0x0B): When the battery level is POWER OFF.

Indicator Command Class


The Receptacle support the Indicator Command Class, version 3 and support the Indicator ID 0x50 (Identify) and Properties ID 0x03, 0x04 and 0x05
Configurable Parameters




	#
	Name
	Size
	Range
	Default
	Description

	1
	SilentOnOff
	1
	0~3
	0
	Control the sound, 00 = On, 03= Off. Default is 00, Sound ON

	2
	RelockOnOff
	1
	0~255
	255
	0x00 = OFF (Stay Open Mode) 0xFF = ON (Auto Lock) Default is 0xFF (Auto Lock Mode)

	3
	RelockTimer
	1
	1~180
	3
	1 to 180 seconds. Default is 03 seconds 

	4
	WrongCode
	1
	0-255
	5
	0 to 255. Default is 5 times

	6
	PressRandom
	1
	0~255
	255
	0xFF = ON Default. 0x00 = OFF (normally utilised for blind user)

	7
	LockOutTime
	1
	10~180
	30
	10 to 180 seconds. Default is 30 seconds

	8
	OpreatingMode
	1
	0~3
	1
	00 = normal mode, will follow Auto Relock parameter 2 setting. Default Mode          
01= Forbidden mode, keypad & RF lockout mode (except Master Code)  
02 = privacy mode, keypad lockout mode but RF unlock will work (Master Code will also still work)  
03 = passage mode, Lock is permanently unlocked

	9 
	DoorLockPair9
	4
	0~16777215
	16777215
	Collect the BLE Mac address of the door lock. Send the first 3 bytes in parameter 9, and the other 3 bytes in parameter 10. Example MAC of lock = A0F769B40DED, send parameter 9 - A0 F7 69, send parameter 10 - B4 0D ED

	10
	DoorLockPair10
	4
	0~16777215
	16777215
	Collect the BLE Mac address of the door lock. Send the first 3 bytes in parameter 9, and the other 3 bytes in parameter 10. Example MAC of lock = A0F769B40DED, send parameter 9 - A0 F7 69, send parameter 10 - B4 0D ED

	11
	OneTouchLock
	1
	0~255
	0
	0x00 = OFF, 0xFF = ON. Default is 0x00 (OFF)

	15
	ResetDefault
	1
	0~1
	0
	01 = Lock will execute Reset to Factory and forget the gateway pairing
00 = Lock will execute Reset to Factory and remember the gateway pairing

	17
	DeadblotFunc
	1
	0~255
	0
	This parameter is only applicable when:
Parameter 8 = normal mode (00)
Parameter 2 = Auto Relock Off (00)

0x00 = Apply deadbolt will lock door, then un-applying it will NOT unlock the door
0xFF = Default setting. Apply deadbolt will lock door, then un-applying it WILL unlock the door again


	18
	DoorPosition
	1
	0~60
	10
	Alarm sounds from Lock when the door is improperly closed into the frame keeper.            
0 to 60 Seconds. Default = 10 second

	20
	DeadblotInstall
	1
	0~255
	255
	
0x00 = No Deadbolt, 0xFF = Yes have Deadbolt, Default = Yes have deadbolt (0xFF)                         Some locks contain optional deadbolt hardware. This parameter is used to determine if one is installed.


	22
	PrivacyMode
	1
	0~255
	255
	0x00 = OFF, 0xFF = ON. Default Is 0x00 (OFF) - If enabled, when extending (applying) the deadbolt the smart deadbolt lock will resort to Forbidden mode (No PIN or RF even if valid cannot access, please note the Master Code can still open the door)


	24
	BLEInterface
	1
	0~255
	0
	
0x00 = OFF, 0Xff = ON. Default Is 0x00 (OFF)


	25
	BleKeyUid25
	4
	0~16777215
	16777215
	
[bookmark: OLE_LINK3]For example: 01 02 03. Set before using


	26
	BleKeyUid26
	4
	0~16777215
	16777215
	For example: 04 05 06. Set before using

	48
	LowBatPercent
	1
	5~50
	10
	This parameter defines a battery level as the “low battery” unit %
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